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İkitelli Organize Sanayi Bölgesi Mah.Atatürk Bulvarı No: 50 / A 34490 Başakşehir / İstanbul / TÜRKİYE


Telefon : +90 212 549 22 52


Faks      : +90 212 549 25 80


Web      : www.emasas.com.tr
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 EMAS ELEKTROTEKNİK MAKİNA    SANAYİ VE TİCARET A.Ş








Technical Specifications: A14B1K11





�





Order Code:�
�
�
�
A14B1K11�
�
�
�
�
�
�
�
Contact Block:�
�
�
�
�
�
�
�
�
�
�
�















�





Technical Information :








Body:


�
�
-Plastic body�
�
�
�
�
�



�
�
�
-Operating Temperature                      �
-15°/+80°C�
�
-Mechanical life                                  �
50.000 operation�
�
-Electrical life                                 �
50.000 operation�
�
-Type of wire connection�
Terminal�
�
-Wire profile�
2,5 mm²�
�






General Specifications : 


 �
�
�
�
-Range of use                      �
 �
AC15-AC1�
�
-Operating voltage                                   �
Ue�
250V AC�
�
-Operating frequency                               �
f�
50Hz�
�
-Operating current                                   �
Ie�
16 (4) A�
�
-Insulation voltage              �
Ui�
300V�
�
-Stroke resistance voltage     �
Uimp�
2,5kV�
�
-Short circuit breaking capacity�
Icn�
1kA�
�
-Insulation Resistance�
 �
10 MΩ min�
�






Electrical Informations :








Standards: 





- TS EN 61058-1
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Electrical Informations :





General Specifications �
�
�
�
Range Of Use�
 �
AC15�
�
Operating Voltage�
Ue�
230V AC�
�
Fregquency�
F�
50Hz�
�
Operating Current�
Ie�
4A�
�
Insulation Resistance �
Ui�
300V�
�
Stroke Resistance Voltage�
Uimp�
2.5kV�
�
Dielectrical Strength�
 �
1500V AC�
�
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