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Technical Specifications : P2AB
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Technical Information :


	Notes:Technical specifications of the contact block mounted in the control boxesBody:
Plastic Body.  
Opportunity of positioning with plates and Badge Bases.


General Specifications 

Operating Temparature 
-5/+40°C
Mechanical life 
0,5 Million (3000 open-close/hour
Electrical Life
0,1 Million (1800 open-close/hour)
C.Block Tightening Torque
0,6-0,8 Nm
C.Block Connection Wire Profile
Min: 1x0,5 mm'2
Wire Profile
Max: 2x2,5 mm'2
Protection Degree
IP50



	


Standards: 

- TS EN 60947 -5-1

In contact Blocks;

- VDE 0660 
-  UL 508		
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	General Specifications 
	
	

	Range Of Use
	 
	AC15

	Operating Voltage
	Ue
	250V AC

	Fregquency
	f
	50Hz

	Operating Current
	Ie
	4A

	Insulation Resistance 
	Ui
	300V

	Stroke Resistance Voltage
	Uimp
	2.5kV

	Dielectrical Strength
	 
	1500V AC


Electrical Informations :
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