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Ziya Gökalp Mah. İkitelli Organize Sanayi Bölgesi Atatürk Bulvarı No:50 34490 Başakşehir / İstanbul / TÜRKİYE


Telefon : +90 212 549 22 52


Faks      : +90 212 549 25 80
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 EMAS ELEKTROTEKNİK MAKİNA    SANAYİ VE TİCARET A.Ş








Technical Specifications : PY1BOŞ
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Series Plastic Control Boxes





Standards: 





- TS EN 60947 -5-1





In Contact Blocks;





- VDE 0660 
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Body:�
�
Plastıc housing.  �
�
Opportunity of positioning with plates and Badge Bases.�
�
�
�
�
General Specifications �
�
�
Operating Temparature �
-5/+83°C�
�
Body Tightening Torque�
 1,5 Nm�
�
Protectıon Degree�
IP65�
�






Technical Information :





Suitable to Ø22 mm buttons                           


 Strong resistance against mechanical strokes through glass fibre reinforced plastic body


5 body types in different dimensions


Usage facility with coloured buttons


Maximum strength to environmental conditions with waterproof body

















Electrical Informations :





General Specifications �
�
�
�
Range Of Use�
 �
AC15�
�
Operating Voltage�
Ue�
230V AC�
�
Fregquency�
F�
50Hz�
�
Operating Current�
Ie�
4A�
�
Insulation Resistance �
Ui�
300V�
�
Stroke Resistance Voltage�
Uimp�
2.5kV�
�
Dielectrical Strength�
 �
1500V AC�
�
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