                  Ziya Gökalp Mah. İkitelli Organize Sanayi Bölgesi Atatürk Bulvarı No:50 34490 Başakşehir / İstanbul / TÜRKİYE
Telefon : +90 212 549 22 52
Faks      : +90 212 549 25 80
Web      : www.emasas.com.tr


[image: ss]
 EMAS ELEKTROTEKNİK MAKİNA    SANAYİ VE TİCARET A.Ş


 


Technical Spesification:EBM06PD12

	
Order Code:

EBM06PD12
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Number of Contacts:

 6P+E




















Technical Information:



Body :
 
-Easy assembly with fixed-not falling screw




General Specificaitons

Operating Temprature
-40/+125°C
Mechnical Life
≥500 120 (op/hour)
Electirical Life 
≥100 240 (op/hour)
Cable Tightening Torque
1,2-1,5 Nm
Wire Profile
2,5 mm²


	Genel Özellikler 


Range of use
 
AC15
Operating Voltage
Ue
400V AC
Insulation Voltage
Ui
690V
Frequency
f
50Hz
Operating Current
Ie
16A
Stroke resistance voltage     
Uimp
6kV
Short circuit breaking capacity
Icn
1kA
Insulation Resistance
 
10 MΩ min
Dielectric Strength (For 1 min.)

3000V

Electrical Information:
Standards: 

- TS EN 61984
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Electrical Informations :
General Specifications 


Range Of Use
 
AC15
Operating Voltage
Ue
230V AC
Fregquency
F
50Hz
Operating Current
Ie
4A
Insulation Resistance 
Ui
300V
Stroke Resistance Voltage
Uimp
2.5kV
Dielectrical Strength
 
1500V AC
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