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Technical Specifications: A14B1K11


	Order Code:

A14B1K11



Contact Block:


















                                                         






Technical Information :



Body:

-Plastic body






-Operating Temperature                      
-15°/+80°C
-Mechanical life                                  
50.000 operation
-Electrical life                                 
50.000 operation
-Type of wire connection
Terminal
-Wire profile
2,5 mm²


Electrical Informations :
General Specifications 


Range Of Use
 
AC15
Operating Voltage
Ue
230V AC
Fregquency
F
50Hz
Operating Current
Ie
4A
Insulation Resistance 
Ui
300V
Stroke Resistance Voltage
Uimp
2.5kV
Dielectrical Strength
 
1500V AC

General Specifications : 
 


-Range of use                      
 
AC15-AC1
-Operating voltage                                   
Ue
250V AC
-Operating frequency                               
f
50Hz
-Operating current                                   
Ie
16 (4) A
-Insulation voltage              
Ui
300V
-Stroke resistance voltage     
Uimp
2,5kV
-Short circuit breaking capacity
Icn
1kA
-Insulation Resistance
 
10 MΩ min

Electrical Informations :

Standards: 

- TS EN 61058-1
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